

1. Connect radio and computer with USB cable if install driver first time; right click to run as administrator to install the USB driver




1. Find a place to store

walkie-talkie-C7000.inf files

1. Wait for the installation successfully





1. When an error occurs, Use the Task Manager to close the software. Repeat steps 1-3 to store the walkie-talkie-C7000.inf files in a different location than before.
2. When the radio is connected, open software, and the following figure appears in the settings-comunication port, which proves that USB driver installation is successful.



**Note that when using GD-73 software, you cannot open other software at the same time.**